The plane must meet the requirements specified in this advisory circular.

The driver must maintain visual contact with the runway.