The aircraft must meet the requirements specified in this advisory circular.

The pilot must maintain visual contact with the runway.